{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":50,"n_cols":4,"rows_kept":50,"merged":[[0,0,1,3],[2,0,2,3],[35,0,37,3],[38,0,38,3],[39,0,40,1],[39,2,40,2],[39,3,40,3],[41,0,43,1],[41,2,43,2],[41,3,43,3],[44,0,44,3],[45,0,45,2],[46,0,48,2],[46,3,48,3],[49,0,51,3]],"flags":["formulas_cached_only"]}
["      第    次  曳引与强制驱动电梯维护保养工作项目（内容）和要求（半月）"]
[]
["维保单位：                                项目名称：        \nWBS/电梯编号：                      当地编号/使用单位编号："]
["序号","维保项目","维保内容","结果"]
[1,"机房、润滑间环境","清洁、门窗完好，照明正常"]
[2,"手动紧急操作装置","齐全、在指定位置"]
[3,"驱动主机","运行时无异常振动和异常声响"]
[4,"制动器各销轴部位","动作灵活"]
[5,"制动器间隙","打开时制动衬和制动轮不应发生摩擦，间隙值符合制造单位要求"]
[6,"制动器作为轿厢意外移动和保护装置制停子系统时的自监测","制动力人工方式检测符合使用使用维护说明书要求；制动力自监测系统有记录"]
[7,"编码器","清洁、安装牢固"]
[8,"限速器各销轴部位","润滑、转动灵活；电气开关正常"]
[9,"层门和轿门旁路装置","工作正常"]
[10,"紧急电动运行","工作正常"]
[11,"轿顶","清洁、防护栏安全可靠"]
[12,"轿顶检修开关、停止装置","工作正常"]
[13,"导靴上油杯","吸油毛毡齐全，油量适宜，油杯无泄露"]
[14,"对重/平衡重块及其压板","对重/平衡重块无松动，压板紧固"]
[15,"井道照明","齐全正常"]
[16,"轿厢照明、风扇、应急照明","工作正常"]
[17,"轿厢检修开关、停止装置","工作正常"]
[18,"轿内报警装置、对讲系统","工作正常"]
[19,"轿内显示、指令按钮","齐全有效"]
[20,"轿门防撞击保护装置（安全、触板、光幕、光电等）","功能有效"]
[21,"轿门门锁电气触点","清洁、触点接触良好，接线可靠"]
[22,"轿门运行","开启和关闭正常工作"]
[23,"轿厢平层准确度","符合标准值"]
[24,"层站召唤、层楼显示","齐全有效"]
[25,"层门地坎","清洁"]
[26,"层门自动关闭装置","正常"]
[27,"层门门锁自动复位","各层门钥匙打开手动开锁装置释放后，层门门锁能自动复位"]
[28,"层门门锁电气触点","清洁、触点接触良好，接线可靠"]
[29,"层门锁紧元件啮合长度","不小于7mm"]
[30,"底坑环境","清洁、无渗水、积水、照明正常"]
[31,"底坑停止装置","工作正常"]
["本次保养工作中发现的问题及需要客户处理的事项："]
[]
[]
["维保单位确认"]
["备注",null,"姓名","日期"]
[]
[]
[]
[]
["使用单位确认"]
["使用单位意见和建议",null,null,"使用单位安全管理人员（签字）"]
[]
[]
[]
["备注：维护保养内容若有增加，可自行添加"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}