{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["电梯维护保养","电梯参数"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"电梯维护保养","index":0,"n_rows":9,"n_cols":11,"rows_kept":9,"merged":[[0,0,0,10],[1,1,1,10],[2,1,2,10],[3,2,3,4],[3,8,3,9],[4,2,4,4],[4,8,4,9],[5,1,5,10],[6,0,7,1],[6,2,7,3],[6,4,8,4],[6,5,6,10],[7,5,7,10],[8,0,8,1],[8,2,8,3],[8,5,8,10]],"flags":["formulas_cached_only"]}
["报价单"]
["询价单位","贵州茅台酒厂（集团）循环经济产业投资开发有限公司"]
["报价须知","1.最高限价：保养费用：20000.00元/年，维修费用：5000.00元/年，维修保养费用总金额不超25000.00元/年，该费用含4台电梯的的所有费用，超过该限价为无效报价；产生的维修项目以实际维修情况据实结算（备注：年度维修费用超过预算5000元，则超过部分发包人重新履行立项程序，在维修过程发现维修清单若有漏项，则发包人组织通过谈价方式确定维修单价）。\n2.本项目无预付款，承包人按照要求完成电梯的季度保养，并经发包人确认后，按照每季度付款一次，本季度发生的维修费用与维护保养费用一起支付。服务期限为三年，一年一考核，合同一年一签；\n3.所报价格包含税金、运费、差旅费、食宿费及工作开展过程中所产生各种费用等。\n4.电梯每月维护保养不得少于2次，全年不得少于24次。每季度维保合格后开具符合国家规定的发票，我公司将每月对维保情况进行确认如未按照要求进行保养，我公司有权按照年维保费用进行折算扣减。\n5.承包人在接到困人故障通知后30分钟内派员到达现场进行处理，非困人故障在2小时内派员到达现场进行处理。配合发包人确保电梯通过当地特种设备检验机构定期检验或检测第三方机构检测。\n6.电梯年检费（每年一次）、限速器校验费(每两年一次)和125%载荷试验费（每五年一次）不包含在上述费用内，由发包人承担。"]
["序  号","名称","规格型号",null,null,"单位","数量","限价    （元/年）","保养费（元/年）",null,"备注"]
[1,"电梯维修保养","蒂森电梯",null,null,"台",4,25000,null,null,"具体参数见附件"]
["合计(元)"]
["报价单位（盖章）",{"$nulls":3},"委托报价人信息","姓名："]
[{"$nulls":5},"证件号码："]
["报价时间",{"$nulls":4},"联系方式："]

{"sheet":"电梯参数","index":1,"n_rows":5,"n_cols":6,"rows_kept":5,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["蒂森电梯"]
[null,"设备名称","型号","技术参数","数量","备注"]
[1,"曳引驱动乘客电梯","thyssenkrupp meta200MR","额定载重：1000kg\n额定速度：1m/s\n层站数：2层2站2门\n控制方式：集选",1,"无机房"]
[2,"曳引驱动乘客电梯","thyssenkrupp meta200MR","额定载重：1000kg\n额定速度：1m/s\n层站数：6层6站6门\n控制方式：集选",2,"有机房"]
[3,"曳引驱动乘客电梯","thyssenkrupp meta200MR","额定载重：1350kg\n额定速度：1m/s\n层站数：4层4站4门\n控制方式：集选",1,"有机房"]